# Waste Management Plan template

**This will assist you and Council officers in identifying the waste and recycling needs of the development.**

Complete and submit this template for proposed developments of five or more residential dwellings with your plan drawings (to scale 1:100 and/or 1:200). Please refer to *Waste Guidelines for new residential and mixed use developments within Cardinia Shire* for assistance in completing this template.

**Planning application number:**

**Address**:

**Land use type**:

**Development description**:

Residential only

**(fill out this section if you have selected residential from the land use type)**

Size of dwellings:
For mixed or other please provide details here:

|  |  |  |  |
| --- | --- | --- | --- |
| **Number of dwellings** | **Garbage(litres per week)** | **Recycling(litres per week)** | **Green waste(litres per week)** |
| Click here to enter number of dwellings. | Click here to enter how much garbage will be generated. | Click here to enter how much recycling will be generated. | Click here to enter how much green waste will be generated. |
| **Total bins proposed:** | Enter number of bins. | Enter number of bins. | Enter number of bins. |
| Note: bin storage and collection points should be clearly marked on your plans.**Space allowance for bulky items/hard waste (m2):** Click here to enter text.**Bin storage locations:** Click here to enter text.**Proposed collection provider:** If **private** you must enter the reason here: Enter reason**Waste collection location:** If **other**, please specify: Click here to enter text. |

### Mixed residential and commercial collections only

### **(fill out this section if you selected mixed use for the land use type)**

Note: Commercial and residential waste should be stored separately.

Description of waste collection bins proposed including location: Click here to enter text.

**Proposed collection provider**:

Note. Council operate 120L garbage and 240L recycle only.

Frequency of collections: Garbage:

 Recycling

 Green waste:
If **other**, please specify: Click here to enter text.

Communal residential waste storage areas only

### **(fill out this section if your application is proposing a communal waste area)**

**Detail storage area ventilation and bin wash area:** Click here to enter text.

**Describe access to communal waste storage area:** Click here to enter text.

**Describe noise minimisation controls:** Click here to enter text.

**Describe waste education arrangements to prevent contamination of recycling and dumping:** Click here to enter text.

**Detail responsible parties and provisions to maintain amenity of the communal storage area.**i.e. *Lease agreement or conditions/Caretaker/manager on-site/owners corporation delegate.* *Click here to enter text.*

**Detail parking arrangements and any parking restrictions on-site for waste collections:**Click here to enter text.

**Describe features for preventing vermin, vandalism and theft of bins:** Click here to enter text.

# Checklist

**Have you checked that:** (select the box to tick off)

[ ]  bins are not placed in turning areas.

[ ]  bins do not interfere with the use of access driveways, loading bays or parking bays.

[ ]  bin collection point is clearly visible or easily identified and not located on a bend in the road

[ ]  designated turning areas have appropriate parking restrictions

**Does your plan show:** (select the box to tick off)

[ ]  vehicles can navigate internal roads & turning circles to AustRoads standard 8.8m service vehicle.

[ ]  vehicles can move in a forward direction without reversing, collecting with a left side arm.

[ ]  size and location of any communal bin storage area.

[ ]  bin storage location when not being presented for collection.

**This waste management plan complies with the following:** (select the box to tick off)

[ ]  overhangs and height clearances are suitable for collection vehicles.

[ ]  access roads to bin collection locations are to the appropriate weight standards.

[ ]  bins presented for collection have 0.5m clearance from another bin or obstruction.